

Shannon, there is some partial blockage in the pipe or Valve of the first part of this piping. So, the left manometer is not showing any movement when pressure is changing even though the right manometer is moving up and down, I hope we can have this fully working by Thursday 6/17

Thanks, Don B